In order to get a grib through winlink on iridium go, do the following:  
  
1. Open RMS express  
2. On winlink screen, click “grib file request” icon ( 2 wind feathers). This will open grib map.   
3. Set grib map parameters you want and click “post request”   
4. In upper right corner of winlink main screen, there is a drop down box (next to “open session”)  
5. On drop down box, choose “Iridium Go winlink”  
6. Click on “open session” . This will open the Iridium Go telnet winlink session screen  
7. Wait for “checking device status” line giving satellite signal information.  
8. Click “start”  
9. Now you wait for connection. Sometimes it loses connection midway through the process, so you have to start over. To do this, wait for Iridium Go to disconnect and wait for “start” to highlight before clicking “start” again. Be patient. This process can take upwards to 45 or more minutes.   
10. Once the grib request post has been sent, you start the process of clicking “Start” to receive the grib chart, which will show up in your inbox.   
11. Click yellow icon in the inbox and that will open the grib file in your Viewfax program.

Thanks John and Leilani on Amazing Grace